# drm_intel_hd &

[1] 790554

# drm_resmgr:  Starting DRM...

[drm:drm_pci_init], 

[drm:drm_get_pci_dev], 

[drm:drm_get_minor], 

[drm:drm_get_minor], new minor assigned 64

[drm:drm_get_minor], 

[drm:drm_get_minor], new minor assigned 0

  Vendor ID: 0x8086

  Device ID: 0x27AC

  Vendor ID: 0x8086

  Device ID: 0x27B9

[drm:init_vbt_defaults], Set default to SSC at 100MHz

[drm:intel_modeset_init], 2 display pipes available.

[drm:intel_crtc_init], swapping pipes & planes for FBC

[drm:intel_modeset_init], plane 0 init failed: -19

[drm:intel_crtc_init], swapping pipes & planes for FBC

[drm:intel_modeset_init], plane 1 init failed: -19

[drm:intel_pch_pll_init], No PCH PLLs on this hardware, skipping initialisation

[drm:drm_edid_block_valid], Fixing EDID header, your hardware may be failing

[drm:drm_edid_block_valid] *ERROR* EDID checksum is invalid, remainder is 130

[drm:drm_edid_block_valid], Fixing EDID header, your hardware may be failing

[drm:drm_edid_block_valid] *ERROR* EDID checksum is invalid, remainder is 130

[drm:drm_edid_block_valid], Fixing EDID header, your hardware may be failing

[drm:drm_edid_block_valid] *ERROR* EDID checksum is invalid, remainder is 130

[drm:drm_edid_block_valid], Fixing EDID header, your hardware may be failing

[drm:drm_edid_block_valid] *ERROR* EDID checksum is invalid, remainder is 130

[drm:intel_lvds_init], using current (BIOS) mode: [drm:drm_mode_debug_printmodeline], Modeline 0:"800x600" 0 40000 800 840 968 1056 600 601 605 628 0x0 0x0

[drm:drm_sysfs_connector_add], adding "LVDS-1" to sysfs

[drm:drm_sysfs_hotplug_event], generating hotplug event

[drm:drm_sysfs_connector_add], adding "VGA-1" to sysfs

[drm:drm_sysfs_hotplug_event], generating hotplug event

[drm:intel_setup_outputs], probing SDVOB

[drm:intel_gmbus_force_bit], enabling bit-banging on i915 gmbus dpb. force bit now 1

[drm:intel_sdvo_read_byte], i2c transfer returned -6

[drm:intel_sdvo_init], No SDVO device found on SDVOB

[drm:intel_gmbus_force_bit], disabling bit-banging on i915 gmbus dpb. force bit now 0

[drm:intel_setup_outputs], probing SDVOC

[drm:intel_gmbus_force_bit], enabling bit-banging on i915 gmbus dpb. force bit now 1

[drm:intel_sdvo_read_byte], i2c transfer returned -6

[drm:intel_sdvo_init], No SDVO device found on SDVOC

[drm:intel_gmbus_force_bit], disabling bit-banging on i915 gmbus dpb. force bit now 0

[drm:drm_sysfs_connector_add], adding "SVIDEO-1" to sysfs

[drm:drm_sysfs_hotplug_event], generating hotplug event

Process 790554 (drm_intel_hd) terminated SIGSEGV code=1 fltno=11 ip=b0340124(/usr/lib/ldqnx.so.2@atomic_set+0x8) mapaddr=00040124. ref=00b42

ff8

[1] + Memory fault         drm_intel_hd  (core dumped)

# 

# 
